Product Name: DSP-AEC-0606,DSP-AEC-1010-DA

FW Version: 10h.2.6.2
Release Date: 2025/09/05

----------------------------------------------------------
1. Prerequisites
----------------------------------------------------------

- DSP needs to be upgraded to minimum 10b.2.2.1 FW before installing this upgrade.


----------------------------------------------------------
2. Revision History
----------------------------------------------------------

FW Version 10h.2.6.2
- Bug fix DSP randomly hangs when using USB.

FW Version 10h.0.2.1
- Adding support for TiGHT AV ASCII based API. Still supporting legacy HEX based V1 and V2 protocols.
- Adding support for TCP control protocol. Port 50000.
- Adding TCP protocol for User Interface external control commands. 
- Various stability improvements.
- Updated TiGHT AV DSP2.0 software.

FW Version 10b.2.2.1 
- Fixes bug when upgrading from DSP V1.0 firmwares.

FW Version: 10b.2.1.1
DSP 2.0 Software compability:
- Enables USB inputs and outputs processing
- Meters now available also for USB inputs and outputs
- Light mode theme added
- Faders will adjust respectively in group mode
- Device snapshot (all device settings and presets) import and export
- Consolidates DSP-AEC-0606, DSP-AEC-1010-DA HW Rev 1 and 2 under same firmware and upgrade tool.

FW Version: 10b.0.5.3 (HW Rev2)
DSP 2.0 Software compability:
- Enables USB inputs and outputs processing
- Meters now available also for USB inputs and outputs
- Light mode theme added
- Faders will adjust respectively in group mode
- Device snapshot (all device settings and presets) import and export


FW Version: 10.0.230414 (HW Rev2)
- Adding support for HW Rev 2 DSP (Colorful re-design and USB 2.0 Type B host port)
- Automatic power cycle after factory reset or firmware upgrade added.

FW Version: 1.0.220914 (HW1)
- Automixer improvements: Priority order settings


FW Version: 1.0.210917 (HW1)
- Production firmware




